CHARCOAL CANISTER, CANISTER VENT (CV) SOLENOID VALVE, AIR FILTER COMPONENT REMOVAL/INSTALLATION [MZI-3.7]

id0116d2819100

1. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [MZI-3.7].)

  Note
  • Remove the charcoal canister, CV solenoid valve, and air filter as a single unit.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

ac9wzw00002193

1 | Under guard (LH)
2 | CV solenoid valve connector
3 | Quick release connector (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [MZI-3.7].)
4 | Quick release connector (See QUICK RELEASE CONNECTOR (EMISSION SYSTEM) REMOVAL/INSTALLATION [MZI-3.7].)
5 | Evaporative hose
6 | Charcoal canister, CV solenoid valve, air filter component