DTC U3003:04 [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE]

id0902q3408100

Description | Instrument cluster configuration error
--- | ---
Detection condition | • Instrument cluster configuration error detected.
Fail-safe function | • Blind spot monitoring (BSM) system is stopped.
Possible cause | • Instrument cluster configuration error • BSM control module malfunction
System wiring diagram | Not applicable

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM INSTRUMENT CLUSTER CONFIGURATION • Using the M-MDS, perform the instrument cluster configuration. (See INSTRUMENT CLUSTER CONFIGURATION.) • Clear the DTC for the BSM control module using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Retrieve the BSM control module DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Is the same DTC displayed? | Yes | Using the M-MDS, perform the instrument cluster configuration again, then go to the next step. (See INSTRUMENT CLUSTER CONFIGURATION.)
No | Go to Step 3.
2 | VERIFY THAT REPAIRS HAVE BEEN COMPLETED • Clear the DTC for the BSM control module using the M-MDS. (See CLEARING DTC [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Retrieve the BSM control module DTCs using the M-MDS. (See DTC INSPECTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) • Is the same DTC displayed? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the BSM control module. (See BLIND SPOT MONITORING (BSM) CONTROL MODULE REMOVAL/INSTALLATION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].) Go to the next step.
No | Go to the next step.
3 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 10-PIN TYPE].)
No | DTC troubleshooting completed.