LIFTGATE LOCK STRIKER REMOVAL/INSTALLATION

id091400804100

1. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

2. Remove the seat side box. (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

3. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

4. Remove the bolts, then remove the liftgate lock striker.

ac9uuw00000552

5. Install in the reverse order of removal.

6. Adjust the liftgate. (See LIFTGATE ADJUSTMENT.)