POWER LIFTGATE (PLG) FRONT SWITCH INSPECTION

id091100002300

1. Disconnect the negative battery cable.

2. Remove the power liftgate (PLG) front switch. (See POWER LIFTGATE (PLG) FRONT SWITCH REMOVAL/INSTALLATION.)

3. Verify that the continuity is as indicated in the table.

ac9wzw00002890

  • If not as indicated in the table, replace the cluster switch. (See CLUSTER SWITCH REMOVAL/INSTALLATION.)

4. Apply battery positive voltage to PLG front switch terminal E, and connect terminal A to ground.

ac9wzw00002684

5. Verify that the LED illuminates.

  • If there is any malfunction, replace the cluster switch.