REAR BUMPER REMOVAL/INSTALLATION

id091000800700

1. Disconnect the negative battery cable.

2. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

3. Remove the screw and fastener.

ac9uuw00000866

4. Detach the tab of the splash shield to remove it.

5. Remove the clip of the rear over fender and put aside the rear bumper.

ac9uuw00002346

6. Remove in the order indicated in the table.

ac9uuw00002630

1 | Fastener A
2 | Fastener B
3 | Protector tape
4 | Screw
5 | Fastener C
6 | Rear bumper (See Rear Bumper Removal Note) (See Rear Bumper Installation Note)

7. Install in the reverse order of removal.

Rear Bumper Removal Note

1. Pull the rear bumper ends (wheel arch) outward (1) to disengage from the bumper slider.

ac9uuw00000868

  Caution
  • When disengaging the rear bumper from the bumper slider, the rear bumper could fall and be damaged. Secure the rear bumper so that it does not fall.

2. Remove the rear bumper (2).

Rear Bumper Installation Note

1. Spread the rear bumper ends apart.

2. Assemble the rear bumper to the body.

3. Press the rear bumper connecting area into the body to engage with the bumper slider.