SHIFT-LOCK INSPECTION

id051800800400

1. Turn the ignition switch to the ON position.

2. Verify that the selector lever is in the P position.

3. Verify that the selector lever cannot be shifted from the P position without depressing the brake pedal.

4. Depress the brake pedal and verify that the selector lever cannot be shifted from the P position.

  • If there is any malfunction, inspect the interlock cable.
  (See INTERLOCK CABLE INSPECTION.)