KEYLESS CONTROL MODULE CONFIGURATION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id0914008068z6

  Note
  • Use the IDS (laptop PC) because the PDS (Pocket PC) does not support the KEYLESS CONTROL MODULE CONFIGURATION.
  • If the configuration is performed using As-Built data, the set value of the personalization function is reset to the initial value (condition when shipped from factory). Verify the set value with the customer and perform the personalization function setting after performing the configuration using As-Built data.

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select “Module Programming”.

3. Then, select items from the screen menu in the following order.

  1. Select “Programmable Module Installation”.
  2. Select “RKE”.

4. Perform the configuration according to the directions on the screen.

5. Retrieve DTCs by the M-MDS, then verify that there is no DTC present.

  Caution
  • When the configuration is performed, CAN communication between the keyless control module and control module connected to the CAN line is cut temporarily, and communication error DTCs may be detected. After performing the configuration, verify the DTCs for the control module connected to the CAN line and clear it if any DTC is detected.

  • If a DTC (s) is detected, perform the applicable DTC inspection. (See DTC TABLE [ADVANCED KEYLESS ENTRY AND START SYSTEM].)