EXTERIOR OPEN/CLOSE FUNCTION OPERATION

id091200102300

• With the function, all doors glass and sunroof can open/close in conjunction with the UNLOCK/LOCK operation of the transmitter, and request switch (with advanced key system).
• One opening operation fully opens (automatic open) all door glass, and close operation operates only when the operation (manual close) is being performed.
• During IG OFF timer operation (power window system operates approx. 40 s after IG OFF), the power window switch operation has priority over the exterior open/close function.
• Auto reverse pinch protection operation has priority when the door glass is obstructed during close operation.
• The BCM sends the signal requiring the open/close operation to the power window control module (power window main switch) based on the signals input from the switches.
• The power window control module (power window main switch) sends open/close operation signal to the power window motor based on the required signal, and operates the door glass.

Open/close Function/operation In Conjunction With Transmitter

• The all door glass and sunroof glass can be opened by holding the button in the UNLOCK position for approx. 2.5 s or more within the transmitter reception area.
• The all door glass and sunroof glass can be closed by holding the button in the LOCK position for approx. 1.5 s or more within the transmitter reception area.

ac9wzn00000619

Close Function/operation In Conjunction With Request Switch

• If the driver-side request switch is operated and held for approx. 1.5 s or more while the transmitter is within the reception area and the all door glass and sunroof glass is open, the all door glass and sunroof glass performs manual close operation. When the switch is released, the operation stops.
• During the operation, when the open/close function in conjunction with the key operation is performed, or the open/close function in conjunction with the transmitter is performed, these functions have priority over the operation.

ac9wzn00000620

Operation Prohibition/stop Condition

• When the following conditions are met before the operation, the exterior open/close function does not operate. Also, if the conditions are met during the operation, the operation stops.

  ― Either door/trunk/liftgate is open (when the door switch or cargo compartment light switch is ON)
  ― The key is inserted in the steering lock (when the keyless switch is ON)
  ― The push button start (ignition switch) is in a position other than the OFF (with advanced key system)
  ― The transmitter is not in the reception area
  ― The transmitter is operated during the operation (LOCK, UNLOCK operation)