MANUAL MODE SHIFT CONTROL OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3225900

• By moving the shift lever from the “D” position into the manual shift position and shifting into + (up-shift) or -(down-shift), the driver can select the desired gear, enabling sporty driving that feels like a manual transaxle. However, the TCM automatically performs upshifting to prevent over-revving, downshifting if vehicle speed decreases, and TCC control.