SIDE GARNISH REMOVAL

id091600804600

Front

1. Pull the side garnish and remove clip A from the vehicle body.

ac9uuw00000494

2. Slide the side garnish to the vehicle rear and remove clips B and C from the side garnish.

3. Remove the side garnish.

4. Remove clips B and C from the body, then install it to the side garnish.

Rear

1. Pull the side garnish and remove clip A from the vehicle body.

ac9uuw00000495

2. Slide the side garnish to the vehicle rear and remove clips B and C from the side garnish.

3. Remove the side garnish.

4. Remove clips B and C from the body, then install it to the side garnish.