POWER WINDOW MAIN SWITCH CONSTRUCTION

id091200007000

• Manual open/close can be performed for all door glasses by operation of the power window main switches.
• Manual open/close can be performed for each specific window by operation of the switches at the all door glasses.
• Auto open/close can be performed for front windows by operation of the power window main switches.
• By locking the power cut switch, operation of the power window main switches for each door glasses and the power window subswitches is inhibited.
• A built-in P/W CM (power window control module) controls the power window system control based on the pulse signals from the power window motor.
• The position and movement direction of the window is stored at the time of vehicle delivery. Due to this, the initial position setting must be performed after performing any of the following procedures:

  ― Disconnecting the negative battery cable.
  ― Removing the power window system power supply fuse.
  ― Disconnecting the power window switch connector.

Block Diagram

ac9wzn00000572