FRONT FOG LIGHT REMOVAL/INSTALLATION

id091800802100

1. Disconnect the negative battery cable.

2. Remove the front under cover B. (See FRONT UNDER COVER REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00002559

4. Remove the screws.

ac9wzw00002560

5. Remove the front fog light and bracket.

ac9wzw00002561

6. Remove the bolt and screw.

ac9wzw00002562

7. Remove the front fog light.

ac9wzw00002563

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When replacing the bulb, hold the metal flange, not the glass.

8. Install in the reverse order of removal.

9. Adjust the front fog light aiming. (See FRONT FOG LIGHT AIMING.)