CONDENSER INSPECTION

id071100801300

1. Inspect the condenser for cracks, damage, and oil leakage.

  • If there is any malfunction, replace the condenser.

2. Visually inspect the fins for clogging of foreign material.

  • If any fins are clogged, remove the foreign material.

3. Visually inspect the fins for bending.

  • If there is any bending, use the end of a flathead screwdriver to straighten fins.