AIR INTAKE ACTUATOR INSPECTION

id074000801500

1. Connect battery positive voltage to air intake actuator terminal G, connect terminal A (or C) to ground, and then verify that the air intake actuator operates as shown in the table.

  • If the operation condition is not normal, replace the air intake actuator.

ac9uuw00002292

ac9wzw00002800

Terminal | Air intake actuator operation
--- | ---
A (C) | C (A) | G
Ground | – | B+ | RECIRCULATE → FRESH
– | Ground | B+ | FRESH → RECIRCULATE

( ): R.H.D.