PID/DATA MONITOR TABLE

id080200800800

PID name (definition) | Unit/Condition | Operation Condition (Reference)
--- | --- | ---
BUCKLE_D (Driver-side buckle switch status) | Unbuckled/Buckled | • Driver-side buckle switch off: Buckled • Driver-side buckle switch on: Unbuckled
BUCKLE_P (Passenger-side buckle switch status) | Unbuckled/Buckled | • Passenger-side buckle switch off: Buckled • Passenger-side buckle switch on: Unbuckled
CCNT_RCM (Number of continuous DTCs) | ― | Indicates number of DTC
IGN_V (IG1 voltage) | V | Ignition switch is at ON: B+
P_BELT_SSR (Occupancy sensor status) | Off/On | • Occupant seated in passenger-side front seat (occupancy sensor on): On • Occupant not seated in passenger-side front seat (occupancy sensor off): Off
PSAB_DepSt (Passenger-side air bag module deployment status) | Inactive/Active | • Passenger-side air bag module non-operation (non-deployment) status: Inactive • Passenger-side air bag module operation (deployment) enabled status: Active
RES_AB_D (Driver-side air bag module resistance) | ohm | Under any condition: 1.39—6.23 ohms
RES_AB_P (Passenger-side air bag module resistance) | ohm | Under any condition: 0.9—6.23 ohms
RES_CAB_D (Driver-side curtain air bag module resistance) | ohm | Under any condition: 0.9—10.36 ohms
RES_CAB_P (Passenger-side curtain air bag module resistance) | ohm | Under any condition: 0.9—10.36 ohms
RES_PT_D (Driver-side pre-tensioner seat belt resistance) | ohm | Under any condition: 0.9—6.23 ohms
RES_PT_P (Passenger-side pre-tensioner seat belt resistance) | ohm | Under any condition: 0.9—6.23 ohms
RES_SAB_D (Driver-side side air bag module resistance) | ohm | Under any condition: 0.9—10.36 ohms
RES_SAB_P (Passenger-side side air bag module resistance) | ohm | Under any condition: 0.9—10.36 ohms