REAR DOOR HINGE REMOVAL/INSTALLATION

id091100520800

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Rear door (See REAR DOOR REMOVAL/INSTALLATION.)

  (2) Front scuff plate (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00003066

1 | Bolt
2 | Nut
3 | Rear door hinge

4. Install in the reverse order of removal.

5. Adjust the front door. (See DOOR ADJUSTMENT.)