DTC INSPECTION [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id09021g345400

1. Connect the M-MDS to the DLC-2.

L.H.D.

ac9uuw00000633

R.H.D.

ac9wzw00000487

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Self Test”.
  2. Select “Modules”.
  3. Select “RKE”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection.

4. After completion of repairs, clear all DTCs stored in the keyless control module. (See CLEARING DTC [ADVANCED KEYLESS ENTRY AND START SYSTEM].)