REAR LATERAL LINK REMOVAL/INSTALLATION

id021400801200

1. When working on the left side of the vehicle, disconnect the rear auto leveling sensor link lower side. (Vehicle with headlight auto leveling system) (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION.)

2. Mark the adjusting cam bolt and cam plate of the rear lateral link.

3. Jack up the rear suspension with unloaded condition.

4. Remove the rear lateral link.

ac9uuw00000933

5. Install the rear lateral link by aligning it with the mark placed during removal.

6. Inspect for rear wheel alignment, and adjust it as necessary. (See REAR WHEEL ALIGNMENT [2WD].) (See REAR WHEEL ALIGNMENT [4WD].)