MICROPHONE REMOVAL/INSTALLATION

id092000801400

1. Disconnect the negative battery cable.

2. Remove the intruder sensor (with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

3. Remove the front map light. (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

4. Press the microphone in the direction indicated by the arrow and remove the microphone.

ac9uuw00000536

5. Install in the reverse order of removal.