FRONT DOOR HINGE REMOVAL/INSTALLATION

id091100520500

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Windshield wiper arm and blade (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

  (2) Side cowl grille (See COWL GRILLE REMOVAL/INSTALLATION.)

  (3) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)

  (4) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

  (5) Sail garnish (See SAIL GARNISH REMOVAL/INSTALLATION.)

  (6) Front fender panel (See FRONT FENDER PANEL REMOVAL/INSTALLATION.)

  (7) Front door (See FRONT DOOR REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9uuw00003063

1 | Bolt A
2 | Front door hinge

4. Install in the reverse order of removal.

5. Adjust the front door. (See DOOR ADJUSTMENT.)