ON-BOARD DIAGNOSTIC SYSTEM DTC TABLE [AY6A-EL, AY6AX-EL]

id0502k1290200

DTC No. | MIL | AT warning light | Definition | Fail-safe | Drive cycle (MIL illuminates) | Self test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | --- | ---
P0220:00 | Illuminate | Illuminate | Accelerator pedal position circuit | X | 1 | C | X | (See DTC P0220:00 [AY6A-EL, AY6AX-EL].)
P0601:00 | Illuminate | Illuminate | Flash ROM error | X | 1 | C | X | (See DTC P0601:00 [AY6A-EL, AY6AX-EL].)
P0603:00 | Illuminate | Illuminate | EEPROM error | X | 1 | C | X | (See DTC P0603:00 [AY6A-EL, AY6AX-EL].)
P0604:00 | Illuminate | Illuminate | RAM error | X | 1 | C | X | (See DTC P0604:00 [AY6A-EL, AY6AX-EL].)
P0702:00 | Illuminate | Illuminate | Linear solenoid driver electrical | X | 1 | C | X | (See DTC P0702:00 [AY6A-EL, AY6AX-EL].)
P0706:00 | Illuminate | Illuminate | TR switch circuit range/performance | X | 1 | C | X | (See DTC P0706:00 [AY6A-EL, AY6AX-EL].)
P0707:00 | Illuminate | Illuminate | TR switch circuit low | X | 1 | C | X | (See DTC P0707:00 [AY6A-EL, AY6AX-EL].)
P0708:00 | Illuminate | Illuminate | TR switch circuit high | X | 1 | C | X | (See DTC P0708:00 [AY6A-EL, AY6AX-EL].)
P0711:00 | Illuminate | Illuminate | TFT sensor circuit range/performance | X | 1 | C | X | (See DTC P0711:00 [AY6A-EL, AY6AX-EL].)
P0712:00 | Illuminate | Illuminate | TFT sensor circuit low | X | 1 | C | X | (See DTC P0712:00 [AY6A-EL, AY6AX-EL].)
P0713:00 | Illuminate | Illuminate | TFT sensor circuit high | X | 1 | C | X | (See DTC P0713:00 [AY6A-EL, AY6AX-EL].)
P0715:00 | Illuminate | Illuminate | Input/turbine speed sensor circuit | X | 1 | C | X | (See DTC P0715:00 [AY6A-EL, AY6AX-EL].)
P0717:00 | Illuminate | Illuminate | Input/turbine speed sensor circuit no signal | X | 1 | C | X | (See DTC P0717:00 [AY6A-EL, AY6AX-EL].)
P0720:00 | Illuminate | Illuminate | VSS circuit | X | 1 | C | X | (See DTC P0720:00 [AY6A-EL, AY6AX-EL].)
P0722:00 | Illuminate | Illuminate | VSS circuit no signal | X | 1 | C | X | (See DTC P0722:00 [AY6A-EL, AY6AX-EL].)
P0727:00 | Illuminate | Illuminate | Engine speed input circuit no signal | X | 1 | C | X | (See DTC P0727:00 [AY6A-EL, AY6AX-EL].)
P0729:00 | Illuminate | Illuminate | Gear 6 incorrect ratio | X | 2 | C | X | (See DTC P0729:00 [AY6A-EL, AY6AX-EL].)
P072D:00 | - | Illuminate | Incorrect gear ratio (1GR with engine brake stuck 2GR/3GR) | X | - | C | X | (See DTC P072D:00 [AY6A-EL, AY6AX-EL].)
P0730:00 | Illuminate | Illuminate | Incorrect gear ratio (1GR with engine brake stuck 4GR) | X | 2 | C | X | (See DTC P0730:00 [AY6A-EL, AY6AX-EL].)
P0731:00 | Illuminate | Illuminate | Gear 1 incorrect ratio | X | 2 | C | X | (See DTC P0731:00 [AY6A-EL, AY6AX-EL].)
P0732:00 | Illuminate | Illuminate | Gear 2 incorrect ratio | X | 2 | C | X | (See DTC P0732:00 [AY6A-EL, AY6AX-EL].)
P0733:00 | Illuminate | Illuminate | Gear 3 incorrect ratio | X | 2 | C | X | (See DTC P0733:00 [AY6A-EL, AY6AX-EL].)
P0734:00 | Illuminate | Illuminate | Gear 4 incorrect ratio | X | 2 | C | X | (See DTC P0734:00 [AY6A-EL, AY6AX-EL].)
P0735:00 | Illuminate | Illuminate | Gear 5 incorrect ratio | X | 2 | C | X | (See DTC P0735:00 [AY6A-EL, AY6AX-EL].)
P073F:00 | - | Illuminate | Incorrect Gear Ratio (1GR with engine brake) | X | - | C | X | (See DTC P073F:00 [AY6A-EL, AY6AX-EL].)
P074A:00 | - | Illuminate | Gear 2 stuck | X | - | C | X | (See DTC P074A:00 [AY6A-EL, AY6AX-EL].)
P074B:00 | - | Illuminate | Gear 3 stuck | X | - | C | X | (See DTC P074B:00 [AY6A-EL, AY6AX-EL].)
P074C:00 | - | Illuminate | Gear 4 stuck | X | - | C | X | (See DTC P074C:00 [AY6A-EL, AY6AX-EL].)
P074D:00 | - | Illuminate | Gear 5 stuck | X | - | C | X | (See DTC P074D:00 [AY6A-EL, AY6AX-EL].)
P074E:00 | - | Illuminate | Gear 6 stuck | X | - | C | X | (See DTC P074E:00 [AY6A-EL, AY6AX-EL].)
P0762:00 | Illuminate | Illuminate | Shift solenoid C stuck on | X | 2 | C | X | (See DTC P0762:00 [AY6A-EL, AY6AX-EL].)
P0766:00 | Illuminate | Illuminate | Shift solenoid D performance or stuck off | X | 2 | C | X | (See DTC P0766:00 [AY6A-EL, AY6AX-EL].)
P0771:00 | Illuminate | Illuminate | Shift solenoid E performance or stuck off | X | 2 | C | X | (See DTC P0771:00 [AY6A-EL, AY6AX-EL].)
P0817:00 | - | Illuminate | Starter lock output signal circuit | - | - | C | X | (See DTC P0817:00 [AY6A-EL, AY6AX-EL].)
P0819:00 | - | Illuminate | Up and down switch to transaxle range correlation | X | - | C | X | (See DTC P0819:00 [AY6A-EL, AY6AX-EL].)
P0867:00 | - | Illuminate | ATF pressure | - | - | C | X | (See DTC P0867:00 [AY6A-EL, AY6AX-EL].)
P0882:00 | Illuminate | Illuminate | TCM B+ low | X | 1 | C | X | (See DTC P0882:00 [AY6A-EL, AY6AX-EL].)
P0883:00 | Illuminate | Illuminate | TCM B+ high | X | 1 | C | X | (See DTC P0883:00 [AY6A-EL, AY6AX-EL].)
P0942:00 | Illuminate | Illuminate | Hydraulic pressure unit (at D position) | X | 2 | C | X | (See DTC P0942:00 [AY6A-EL, AY6AX-EL].)
P0961:00 | Illuminate | Illuminate | Line pressure control solenoid circuit range/performance | X | 1 | C | X | (See DTC P0961:00 [AY6A-EL, AY6AX-EL].)
P0962:00 | Illuminate | Illuminate | Line pressure control solenoid circuit low | X | 1 | C | X | (See DTC P0962:00 [AY6A-EL, AY6AX-EL].)
P0963:00 | Illuminate | Illuminate | Line pressure control solenoid circuit high | X | 1 | C | X | (See DTC P0963:00 [AY6A-EL, AY6AX-EL].)
P0973:00 | Illuminate | Illuminate | Shift solenoid A circuit low | X | 1 | C | X | (See DTC P0973:00 [AY6A-EL, AY6AX-EL].)
P0974:00 | Illuminate | Illuminate | Shift solenoid A circuit high | X | 1 | C | X | (See DTC P0974:00 [AY6A-EL, AY6AX-EL].)
P0976:00 | Illuminate | Illuminate | Shift solenoid B circuit low | X | 1 | C | X | (See DTC P0976:00 [AY6A-EL, AY6AX-EL].)
P0977:00 | Illuminate | Illuminate | Shift solenoid B circuit high | X | 1 | C | X | (See DTC P0977:00 [AY6A-EL, AY6AX-EL].)
P0978:00 | Illuminate | Illuminate | Shift solenoid C circuit range/performance | X | 1 | C | X | (See DTC P0978:00 [AY6A-EL, AY6AX-EL].)
P0979:00 | Illuminate | Illuminate | Shift solenoid C circuit low | X | 1 | C | X | (See DTC P0979:00 [AY6A-EL, AY6AX-EL].)
P0980:00 | Illuminate | Illuminate | Shift solenoid C circuit high | X | 1 | C | X | (See DTC P0980:00 [AY6A-EL, AY6AX-EL].)
P0981:00 | Illuminate | Illuminate | Shift solenoid D circuit range/performance | X | 1 | C | X | (See DTC P0981:00 [AY6A-EL, AY6AX-EL].)
P0982:00 | Illuminate | Illuminate | Shift solenoid D circuit low | X | 1 | C | X | (See DTC P0982:00 [AY6A-EL, AY6AX-EL].)
P0983:00 | Illuminate | Illuminate | Shift solenoid D circuit high | X | 1 | C | X | (See DTC P0983:00 [AY6A-EL, AY6AX-EL].)
P0984:00 | Illuminate | Illuminate | Shift solenoid E circuit range/performance | X | 1 | C | X | (See DTC P0984:00 [AY6A-EL, AY6AX-EL].)
P0985:00 | Illuminate | Illuminate | Shift solenoid E circuit low | X | 1 | C | X | (See DTC P0985:00 [AY6A-EL, AY6AX-EL].)
P0986:00 | Illuminate | Illuminate | Shift solenoid E circuit high | X | 1 | C | X | (See DTC P0986:00 [AY6A-EL, AY6AX-EL].)
P0997:00 | Illuminate | Illuminate | Shift solenoid F circuit range/performance | X | 1 | C | X | (See DTC P0997:00 [AY6A-EL, AY6AX-EL].)
P0998:00 | Illuminate | Illuminate | Shift solenoid F circuit low | X | 1 | C | X | (See DTC P0998:00 [AY6A-EL, AY6AX-EL].)
P0999:00 | Illuminate | Illuminate | Shift solenoid F circuit high | X | 1 | C | X | (See DTC P0999:00 [AY6A-EL, AY6AX-EL].)
P1700:00 | - | Illuminate | Hydraulic pressure unit (at R position) | X | - | C | X | (See DTC P1700:00 [AY6A-EL, AY6AX-EL].)
P1719:00 | - | - | Engine torque signal error (inaccurate signal) | X | - | C | X | (See DTC P1719:00 [AY6A-EL, AY6AX-EL].)
P1738:00 | - | Illuminate | Shift control solenoid component malfunction | X | - | C | X | (See DTC P1738:00 [AY6A-EL, AY6AX-EL].)
P1783:00 | - | - | ATF high oil temperature malfunction | X | - | C | X | (See DTC P1783:00 [AY6A-EL, AY6AX-EL].)
P1919:00 | - | - | Engine coolant temperature signal error | X | - | C | X | (See DTC P1919:00 [AY6A-EL, AY6AX-EL].)
P2544:00 | Illuminate | Illuminate | Engine torque signal error (invalid signal) | X | 1 | C | X | (See DTC P2544:00 [AY6A-EL, AY6AX-EL].)
P2708:00 | Illuminate | Illuminate | Shift solenoid F stuck on | X | 2 | C | X | (See DTC P2708:00 [AY6A-EL, AY6AX-EL].)
P2757:00 | Illuminate | Illuminate | TCC control solenoid circuit performance or stuck off | X | 2 | C | X | (See DTC P2757:00 [AY6A-EL, AY6AX-EL].)
P2762:00 | Illuminate | Illuminate | TCC control solenoid range/performance | X | 1 | C | X | (See DTC P2762:00 [AY6A-EL, AY6AX-EL].)
P2763:00 | Illuminate | Illuminate | TCC control solenoid circuit high | X | 1 | C | X | (See DTC P2763:00 [AY6A-EL, AY6AX-EL].)
P2764:00 | Illuminate | Illuminate | TCC control solenoid circuit low | X | 1 | C | X | (See DTC P2764:00 [AY6A-EL, AY6AX-EL].)
P2806:00 | - | Illuminate | Neutral position learning (Not performed yet) | X | - | C | X | (See DTC P2806:00 [AY6A-EL, AY6AX-EL].)
U0073:00 | Illuminate | Illuminate | Control module communication bus off | X | 1 | C | X | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100:00 | Illuminate | Illuminate | Lost communication with PCM | X | 1 | C | X
U0121:00 | - | Illuminate | Lost communication with DSC/RSC HU/CM | X | - | C | X
U0155:00 | - | - | Lost communication with instrument cluster | X | - | C | X
U0415:00 | - | - | Invalid data received from DSC/RSC HU/CM | X | - | C | X | (See DTC U0415:00 [AY6A-EL, AY6AX-EL].)

*1 :C; CMDTC self-test