PID/DATA MONITOR TABLE [POSITION MEMORY CONTROL SYSTEM]

id0902z8979200

—: Not applicable

PID Name (Definition) | Unit/Condition | Operation Condition | Terminal
--- | --- | --- | ---
VPWR | V | Module Supply Voltage | 1F
MIR_SW_UP | ― | Power outer mirror switch (Up) | 2A
MIR_SW_DN | ― | Power outer mirror switch (Down) | 2A
MIR_SELESW_L | ― | Power outer mirror switch (Select the left side mirror) | 2B
MIR_SELESW_R | ― | Power outer mirror switch (Select the right side mirror) | 2B
MIR_SW_L | ― | Power outer mirror switch (Left) | 2C
MIR_SW_R | ― | Power outer mirror switch (Right) | 2C
MIR_MTR_R_V | ― | Right side power outer mirror motor (Up) | 2M
MIR_MTR_R_C | ― | Right side power outer mirror motor (Right / Down) | 2O
MIR_MTR_R_H | ― | Right side power outer mirror motor (Left) | 2Q
MIR_MTR_L_V | ― | Left side power outer mirror motor (Up) | 2S
MIR_MTR_L_C | ― | Left side power outer mirror motor (Right / Down) | 2U
MIR_MTR_L_H | ― | Left side power outer mirror motor (Left) | 2W
SLIDE_SW_F | ― | Slide Switch (Forward) | 3A
SLIDE_SW_B | ― | Slide Switch (Backward) | 3B
FTLT_SW_UP | ― | Front Tilt Switch (Up) | 3C
FTLT_SW_DN | ― | Front Tilt Switch (Down) | 3D
RTLT_SW_UP | ― | Rear Tilt Switch (Up) | 3E
RTLT_SW_DN | ― | Rear Tilt Switch (Down) | 3F
REC_SW_UP | ― | Recline Switch (Up) | 3G
REC_SW_DWN | ― | Recline Switch (Down) | 3H
M_SET_SW | ― | Memory Set Switch | 3K
MEMORY_SW_1 | ― | Memory Switch 1 | 3L
MEMORY_SW_2 | ― | Memory Switch 2 | 3M
MEMORY_SW_3 | ― | Memory Switch 3 | 3N
SLIDE_MTR_F | ― | Slide Motor (Forward) | 4A
SLIDE_MTR_B | ― | Slide Motor (Backward) | 4B
FTLT_MTR_UP | ― | Front Tilt Motor (Up) | 4C
FTLT_MTR_DN | ― | Front Tilt Motor (Down) | 4D
RTLT_MTR_UP | ― | Rear Tilt Motor (Up) | 4E
RTLT_MTR_DN | ― | Rear Tilt Motor (Down) | 4F
REC_MTR_FW | ― | Recline Motor (Forward) | 4G
REC_MTR_BK | ― | Recline Motor (Backward) | 4H