DTC INSPECTION [FORWARD SENSING CAMERA (FSC)]

id0902p9029200

1. Connect the M-MDS to the DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  (1) Select “Self Test”.

  (2) Select “Modules”.

  (3) Select “FSC”.

3. Verify the DTC according to the directions on the screen.

  • If any DTCs are displayed, perform troubleshooting according to the corresponding DTC inspection after recording the snapshot data.

4. After completion of repairs, clear all DTCs stored in the forward sensing camera (FSC). (See CLEARING DTC [FORWARD SENSING CAMERA (FSC)].)

Snapshot Data

• The data for all DTCs currently detected is stored.

—: Not applicable

Snapshot data item | Unit | Data contents | Data read/use method | Corresponding data monitor items
--- | --- | --- | --- | ---
ECU_IN_TMP | °C | °F | ECU internal temperature | — | —
IG-ON_TIMER | hh:mm:ss | Elapsed time since ignition switch was turned to the ON position Note • The instrument cluster records the elapsed time since the ignition switch was turned to the ON position. | When a DTC is detected, the forward sensing camera (FSC) receives the elapsed time since the ignition switch was turned to the ON position being detected by the instrument cluster via CAN signals and displays it in the M-MDS. | —
OPE_MODE | Normal/CALIBRATION/EMERGENCY | Operation mode | — | —
VSPD | KPH | MPH | Vehicle speed | — | VSPD