DTC B2477 [INSTRUMENT CLUSTER]

id0902e8840500

Description | Instrument cluster configuration error
--- | ---
Detection condition | • Instrument cluster configuration has not been correctly performed.
Possible cause | • Instrument cluster configuration error • Instrument cluster malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM INSTRUMENT CLUSTER CONFIGURATION • Perform the instrument cluster configuration using the M-MDS. (See INSTRUMENT CLUSTER CONFIGURATION.) • Clear the DTC for the instrument cluster using the M-MDS. (See CLEARING DTC [INSTRUMENT CLUSTER].) • Retrieve the instrument cluster DTCs using the M-MDS. (See DTC INSPECTION [INSTRUMENT CLUSTER].) • Is the same DTC displayed? | Yes | Perform the instrument cluster configuration again, then go to the next step. (See INSTRUMENT CLUSTER CONFIGURATION.)
No | Go to Step 3.
2 | VERIFY DTC TROUBLESHOOTING COMPLETED • Clear the DTC for the instrument cluster using the M-MDS. (See CLEARING DTC [INSTRUMENT CLUSTER].) • Retrieve the instrument cluster DTCs using the M-MDS. (See DTC INSPECTION [INSTRUMENT CLUSTER].) • Is the same DTC displayed? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the instrument cluster. (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.) Go to the next step.
No | Go to the next step.
3 | VERIFY IF OTHER DTCs DISPLAYED • Are any other DTCs displayed? | Yes | Repair or replace the malfunctioning part according to the applicable DTC troubleshooting. (See DTC TABLE [INSTRUMENT CLUSTER].)
No | DTC troubleshooting completed.