POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION

id091200003500

Mirror Glass Adjustment Switch, Left/right Selection Switch

  Note
  • The mirror glass adjustment switch, left/right selection switch is integrated with the power window main switch. (See POWER WINDOW MAIN SWITCH REMOVAL/INSTALLATION.)

Retractable Outer Mirror Switch

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the bonnet release lever. (See BONNET LATCH AND RELEASE LEVER REMOVAL/INSTALLATION.)

4. Pull the retractable outer mirror switch in the direction of the arrow (2) shown in the figure while pressing the tab in the direction of the arrow (1) shown in the figure, detach the tab and lower panel, and then remove the retractable outer mirror switch from the lower panel.

ac9wzw00002988

5. Disconnect the connector.

6. Install in the reverse order of removal.