DIFFERENTIAL OIL REPLACEMENT

id031400800200

1. Place the vehicle on level ground.

2. Remove the filler plug and the washer.

ac9uuw00001462

3. Remove the drain plug and drain the differential oil into a container.

4. Install a new washer and the drain plug, and tighten.

  Tightening torque

  39.2—53.9 N·m {4.00—5.49 kgf·m, 29.0—39.7 ft·lbf}

5. Add the specified differential oil from the filler plug until the level reaches the brim of the plug hole.

  Rear differential oil

  Specified oil grade: API service GL-5
  Specified oil viscosity: SAE 80W-90
  Capacity (approx quantity): 1.0 L {1.1 US qt, 0.9 Imp qt}

6. After filling with differential oil, perform oil level inspection.

7. Install a new washer and the filler plug, and tighten.

  Tightening torque

  39.2—53.9 N·m {4.00—5.49 kgf·m, 29.0—39.7 ft·lbf}