CLEARING DTC [AUDIO]

id0902f6855600

  Caution
  • If the memory is cleared, past malfunctions may no longer be displayed, therefore before clearing DTCs, record all DTCs displayed in the DTC inspection on the Audio Repair Order Form.

When using the M-MDS

1. Connect the M-MDS to the DLC-2.

2. After vehicle identification, select the following from the M-MDS initialization screen.

  1. “Self-test”
  2. “Module”
  3. “ACU”

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Turn the ignition switch to the OFF position.

6. Turn the ignition switch to the ON position and wait for 5 s or more.

7. Perform DTC inspection. (See DTC INSPECTION [AUDIO].)

8. Verify that no DTCs are displayed.

Not using M-MDS (on-board diagnostic test mode)

1. Turn the ignition switch to the ACC or ON position.

2. Launch the on-board diagnostic test mode. (See DTC INSPECTION [AUDIO].)

3. Select the DTC and press the CLEAR button to clear the DTC.

ac9wzw00002923

4. Turn the ignition switch to the OFF position to complete the on-board diagnostic test mode.