AIR INTAKE CONTROL OPERATION

id074000103500

Air Intake Automatic Control

• The front climate control unit calculates the air intake actuator opening angle (air intake mode) based on the target temperature operating the actuator.

ac9uun00000236

Correction

MAX HOT and MAX COLD correction
• When the set temperature is at 32.0 or 15.0, the air intake is set as shown in the table.

TEMPERATURE CONTROL DIAL | AIR INTAKE MODE
--- | ---
DRIVER SIDE | PASSENGER SIDE
15.0 | 15.0 | REC
15.0 | EXCEPT 15.0, 32.0 | REC
EXCEPT 15.0, 32.0 | 15.0 | REC
32.0 | EXCEPT 15.0, 32.0 | FRESH
EXCEPT 15.0, 32.0 | 32.0 | FRESH
15.0 | 32.0 | FRESH
32.0 | 15.0 | FRESH
32.0 | 32.0 | FRESH

Defroster correction
• When the defroster switch is turned on or the airflow mode is switched to HEAT/DEF mode, the air intake mode switches to fresh air to improve defrosting.

Air Intake Manual Control

• The air intake modes can be switched by operating the REC switch.

Air intake mode | REC switch operation
--- | ---
FRESH | Fixed to FRESH when the REC switch is turned on during REC mode.
REC | Fixed to REC when the REC switch is turned on during FRESH mode.