SUNROOF MOTOR REMOVAL/INSTALLATION

id091500805000

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (6) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (8) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (9) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (14) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (15) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (18) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (19) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (20) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (21) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (22) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

3. Remove the sunroof seaming welt.

4. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION.)

5. Disconnect the sunroof motor connector.

ac9wzw00001576

6. Remove the screws, and then remove the sunroof motor.

7. Install in the reverse order of removal.

  Note
  • If the glass panel or the sunroof motor is moved with the sunroof motor removed, initial position setting of the sunroof motor will be required. Perform initial position setting referring to the Sunroof Motor Assembly Note. (See SUNROOF UNIT DISASSEMBLY/ASSEMBLY.)