DLC-2 CONSTRUCTION

id030200108700

• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.
• Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this connector. The 16-pin connector consists of a CAN_H (HS) terminal, CAN_L (HS) terminal, CAN_H (MS) terminal, CAN_L (MS) terminal, GND1 terminal, GND2 terminal, and B+ terminal.

am5ezn00000934

Terminal | Function
--- | ---
A | Battery power supply terminal
B | -
C | -
D | -
E | Serial communication Lo terminal (HS)
F | Serial communication Hi terminal (HS)
G | -
H | Serial communication ground terminal
I | -
J | Body ground terminal
K | Serial communication Lo terminal (MS)
L | Serial communication Hi terminal (MS)
N | -
M | -
O | -
P | -