WINDSHIELD WASHER HOSE REMOVAL/INSTALLATION

id091900802100

1. Remove the splash shield (RH). (See SPLASH SHIELD REMOVAL/INSTALLATION.)

2. Disconnect windshield washer hose A from the windshield washer motor.

ac9wzw00002608

3. Remove windshield washer hose A from clip A.

4. Disconnect joint pipe A and remove windshield washer hose A.

5. Detach clips B.

6. Disconnect joint pipe A and B and remove windshield washer hose B.

7. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

8. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

9. Remove windshield washer hose C from hook A.

ac9wzw00001604

10. Disconnect joint pipe B and C, than remove windshield washer hose C.

11. Disconnect joint pipe C and remove windshield washer hose D.

12. Disconnect windshield washer hose E from the windshield washer nozzle.

13. Disconnect joint pipe D and remove windshield washer hose E.

14. Remove the windshield washer hose F from the hooks B.

15. Disconnect windshield washer hose F from the windshield washer nozzle.

16. Disconnect joint pipe D and remove windshield washer hose F.

17. Install in the reverse order of removal.