NO.27 FUEL REFILL CONCERNS [MZI-3.7]

id0103d2803300

27 | FUEL REFILL CONCERNS
--- | ---
DESCRIPTION | • Fuel tank is not filled smoothly.
POSSIBLE CAUSE | • Clogged EVAP pipes • Nonreturn valve malfunction • Improper use of fuel nozzle • Inadequate fuel filling speed Warning • The following troubleshooting flow chart contains the fuel system diagnosis and repair procedures. Read the following warnings before servicing the fuel system: ― Fuel vapor is hazardous. It can easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel. ― Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete “BEFORE SERVICE PRECAUTION” and “AFTER SERVICE PRECAUTION” described in this manual. (See BEFORE SERVICE PRECAUTION [MZI-3.7].) (See AFTER SERVICE PRECAUTION [MZI-3.7].) Caution • Disconnecting/connecting quick release connector without cleaning it may cause damage to fuel pipe and quick release connector. Always clean quick release connector joint area before disconnecting/connecting, and make sure that it is free of foreign material.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Turn the ignition switch to the ON position (Engine off). Retrieve any PCM DTCs using the M-MDS. (See ON-BOARD DIAGNOSTIC TEST [MZI-3.7].) Are there any DTCs displayed? | Yes | DTC is displayed: • Go to the appropriate DTC inspection. (See DTC TABLE [MZI-3.7].)
No | No DTC is displayed: • Go to the next step.
2 | Remove the fuel-filler pipe. Make sure the nonreturn valve is installed properly. Inspect the nonreturn valve operation. Is the nonreturn valve normal? | Yes | Inspect for the following: • Improper use of fuel nozzle • Inadequate fuel filling speed Repair or replace the malfunctioning part according to the inspection results.
No | Nonreturn valve is installed improperly: • Reinstall the nonreturn valve to proper position. Nonreturn valve does not operate properly: • Replace the nonreturn valve.
3 | • Verify test results. ― If normal, return to diagnostic index to service any additional symptoms. (See SYMPTOM DIAGNOSTIC INDEX [MZI-3.7].) ― If malfunction remains, inspect related Service Information and perform repair or diagnosis. • If vehicle is repaired, troubleshooting completed. • If vehicle is not repaired or additional diagnostic information is not available, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].)