SUSPENSION SPECIFICATIONS

id020000100300

Suspension

Item | Specification
--- | ---
Front suspension | Type | Strut type
Spring type | Coil spring
Shock absorber type | Low-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 2WD: 31 {1.22} 4WD: 32 {1.25}
Wheel alignment (Unloaded*1) | Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
Degree | 0°09′±0°18′
Maximum steering angle [Tolerance ±3°] | Inner | 38°00′
Outer | 32°00′
Caster angle*2 [Tolerance ±1°] | 2WD: 3°04′ 4WD: 3°05′
Camber angle*2 [Tolerance ±1°] | -0°21′
Steering axis inclination (Reference value) | 11°35′
Rear suspension | Type | Multi-link
Spring type | Coil spring
Shock absorber type | Low-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 2WD: 16 {0.63} 4WD: 18 {0.71}
Wheel alignment (Unloaded*1) | Total toe-in | Tire [Tolerance ±4 {0.16}] | (mm {in}) | 2 {0.08}
Rim inner [Tolerance ±3 {0.12}] | Vehicle equipped with 18 inch wheel: 1.2 {0.047} Vehicle equipped with 20 inch wheel: 1.4 {0.055}
Degree | 0°09′±0°18′
Camber angle*2 [Tolerance ±1°] | 2WD: -0°32′ 4WD: -0°33′
Thrust angle [Tolerance ±0°48′] | 0°

*1 :Unloaded: Fuel tank is full. Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
*2 :Difference between left and right not exceed 1°30′.

Wheel and Tire

Standard tire

Item | Specification
--- | ---
Tire | Size | 245/60R18 104H | 245/50R20 102V
Wheel | Size | 18 x 7 1/2J | 20 x 7 1/2J
Material | Aluminum alloy
Inset | (mm {in}) | 45 {1.8}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

Spare tire

Item | Specification
--- | ---
Tire | Size | 195/80R17 99M
Wheel | Size | 17 x 5 1/2J
Material | Steel
Inset | (mm {in}) | 45 {1.8}
Pitch circle diameter | (mm {in}) | 114.3 {4.5}