CONTROL SYSTEM OUTLINE

id094000103000

• A controller area network (CAN) system has been adopted in which multiple signals are transmitted over a single communication path as a result of wiring harness simplification.
• With an on-board diagnostic function included for each multiplex module, display of DTCs using the Mazda Modular Diagnostic System (M-MDS) has improved serviceability.
• Body control module (BCM) has been adopted.