AUTO LIGHT/WIPER CONTROL MODULE REMOVAL/INSTALLATION

id091800809400

  Caution
  • When replacing the auto light/wiper control module, the configuration procedure must be performed before removing the auto light/wiper control module. Replacing the auto light/wiper control module without performing the configuration procedure will result in system malfunction.

  Note
  • Auto light-off system are integrated with the auto light/wiper control module.

1. Perform the auto light/wiper control module configuration when replacing it. (See AUTO LIGHT/WIPER CONTROL MODULE CONFIGURATION.)

2. Disconnect the negative battery cable.

3. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

4. Remove the parking sensor buzzer. (See PARKING SENSOR BUZZER REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

ac9wzw00005566

1 | Bolt
2 | Connector
3 | Auto light/wiper control module

6. Install in the reverse order of removal.