VARIABLE VALVE TIMING ACTUATOR REMOVAL/INSTALLATION [MZI-3.7]

id0110c5801100

  Warning
  • Fuel vapor is hazardous. It can very easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injures or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete the “Fuel Line Safety Procedure”. (See BEFORE SERVICE PRECAUTION [MZI-3.7].)
  • Continuous exposure to USED engine oil has caused skin cancer in laboratory mice. Protect your skin by washing with soap and water immediately after working with engine oil.

  Caution
  • The variable valve timing actuator cannot be disassembled because it is a precision unit.

  Note
  • The following procedure “VARIABLE VALVE TIMING ACTUATOR REMOVAL/INSTALLATION” is performed after the engine and transaxle component is removed from the vehicle. (See ENGINE REMOVAL/INSTALLATION [MZI-3.7].)

1. Drain the engine oil. (See ENGINE OIL REPLACEMENT [MZI-3.7].)

2. Remove the engine and transaxle component. (See ENGINE REMOVAL/INSTALLATION [MZI-3.7].)

3. Secure the engine and transaxle component using a hoist and the SST.

  Warning
  • Protect and stabilize the lowered engine and transaxle component with crossties to prevent injury or damage due to roll over.

ac9wzw00002218

4. Remove the dynamic chamber and throttle body as a single unit. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZI-3.7].)

5. Remove the ignition coils. (See IGNITION COIL REMOVAL/INSTALLATION [MZI-3.7].)

6. Remove the dipstick.

7. Remove the power steering oil pump drive belt. (See DRIVE BELT REMOVAL/INSTALLATION [MZI-3.7].)

8. Remove the power steering oil pump. (See POWER STEERING OIL PUMP REMOVAL/INSTALLATION [L.H.D.].)(See POWER STEERING OIL PUMP REMOVAL/INSTALLATION [R.H.D.].)

9. Remove the OCV component (LH) (RH). (See TIMING CHAIN REMOVAL/INSTALLATION [MZI-3.7].)

10. Remove in the order indicated in the table.

11. Install in the reverse order of removal.

12. Start the engine and:

  (1) Inspect the runout and contact on the pulley and belt.

  (2) Inspect for engine oil, engine coolant, ATF, power steering fluid and fuel leakage.

  (3) Verify the ignition timing, idle speed and idle mixture. (See ENGINE TUNE-UP [MZI-3.7].)

  (4) Engine accessories operation.

13. Perform a road test.

ac9wzw00003266

1 | Timing chain component (See Timing chain Component Removal Note.) (See Variable Valve Timing Actuator Component Installation Note.)
2 | Variable valve timing actuator component (LH) (See Variable Valve Timing Actuator Component Removal Note.) (See Variable Valve Timing Actuator Component Installation Note.)
3 | Variable valve timing actuator component (RH) (See Variable Valve Timing Actuator Component Removal Note.) (See Variable Valve Timing Actuator Component Installation Note.)

Timing chain Component Removal Note

  Caution
  • When removing the timing chain and marking the timing marks on the chain, mark the camshaft timing chain as well.
  • Do not rotate the crankshaft counterclockwise. The timing chains may bind, causing engine damage.

1. Turn the crankshaft clockwise so that the crankshaft keyway is in the 11 o’clock position. (This will position the No.1 cylinder at TDC.)

ac9wzw00003267

  Note
  • Verify that there are timing marks in four locations on the timing chain. If any timing marks are missing, mark the timing chain.
  • When marking the variable valve timing actuator (RH) side timing chain, change the mark color.
  • When the timing chain is replaced with a new one, mark the new timing chain at the same positions as the removed timing chain.

2. Mark the timing chain at the position of each timing sprocket timing mark.

azzjjw00000157

  Caution
  • Verify that there are timing marks in two locations on the camshaft timing chain. If any timing marks are missing, mark the camshaft timing chain.
  • If replacing with a new variable valve timing actuator, place alignment marks in the same positions as those prior to the replacement.

3. Mark the camshaft timing chain at the positions where it is aligned with each of the camshaft sprocket on both banks.

LH

ac9wzw00002222

RH

ac9wzw00002223

4. Remove the timing chain in the following order.

  (1) Chain tensioner

  (2) Timing chain

  (3) Tensioner arm

  (4) Chain guide

  (5) Crankshaft sprocket

  ac9wzw00002224

Variable Valve Timing Actuator Component Removal Note

1. Rotate the crankshaft counterclockwise until the keyway is in the 9 o'clock position.

ac9wzw00002225

2. Slowly compress the camshaft timing chain tensioner (LH) piston by hand.

3. Insert an approx. 1.0 mm {0.039 in} thin wire or paper clip into the camshaft timing chain tensioner (LH) shown in the figure to hold the tensioner piston.

ac9wzw00002226

  Note
  • When the timing chain removed, valve spring pressure will rotate the camshaft (LH) approx. 3 ° to a neutral position.

4. Install the SST onto the camshafts (LH).

ac9wzw00002227

  Caution
  • Always use an appropriate tool (TORX or TORX PLUS). If the appropriate tool is not used, it could result in damage to the bolts or the tools.

  ac9wzw00003272

  Tool size

  TORX: T55
  TORX PLUS: 55IP

  Note
  • The camshaft sprocket is integrated with the variable valve timing actuator and cannot be disassembled.

5. Remove the variable valve timing actuator, camshaft timing chain and the exhaust camshaft sprocket of the LH bank as a single unit using the appropriate tools.

6. Remove the SST from the camshafts (LH).

7. Slowly compress the camshaft timing chain tensioner (RH) piston by hand.

8. Insert an approx. 1.0 mm {0.039 in} thin wire or paper clip into the camshaft timing chain tensioner (RH) shown in the figure to hold the tensioner piston.

ac9wzw00002229

9. Install the SST onto the camshafts (RH).

ac9wzw00002230

  Note
  • The camshaft sprocket is integrated with the variable valve timing actuator and cannot be disassembled.

10. Remove the variable valve timing actuator, camshaft timing chain and the exhaust camshaft sprocket of the RH bank as a single unit using the appropriate tools.

11. Remove the SST from the camshafts (RH).

Variable Valve Timing Actuator Component Installation Note

1. Align the alignment marks on the camshaft timing chain and both intake and exhaust side camshaft sprockets of both banks.

RH

ac9wzw00005860

LH

ac9wzw00002232

2. Install the variable valve timing actuator, camshaft timing chain and the exhaust camshaft sprocket of the RH bank as a single unit.

3. Remove the retaining wire inserted into the camshaft timing chain tensioner (RH).

ac9wzw00002233

  Caution
  • Always use an appropriate tool (TORX or TORX PLUS). If the appropriate tool is not used, it could result in damage to the bolts or the tools.

  ac9wzw00003272

  Tool size

  TORX: T55
  TORX PLUS: 55IP

4. Tighten the new camshaft sprocket (RH) installation bolts using the appropriate tools following 4 steps.

  (1) Tighten to 40 N·m {4.1 kgf·m, 30 ft·lbf}.

  (2) Loosen 360 ° (one full turn) in reverse order.

  (3) Tighten to 10 N·m {102 kgf·cm, 89 in·lbf}.

  (4) Tighten to 90 °

5. Install the variable valve timing actuator, camshaft timing chain and the exhaust camshaft sprocket of the LH bank as a single unit.

6. Remove the retaining wire inserted into the camshaft timing chain tensioner (LH).

ac9wzw00002234

7. Tighten the new camshaft sprocket (LH) installation bolts using the appropriate tools following 4 steps.

  (1) Tighten to 40 N·m {4.1 kgf·m, 30 ft·lbf}.

  (2) Loosen 360 ° (one full turn) in reverse order.

  (3) Tighten to 10 N·m {102 kgf·cm, 89 in·lbf}.

  (4) Tighten to 90 °

8. Turn the crankshaft clockwise so that the crankshaft keyway is in the 11 o’clock position. (This will position the No.1 cylinder at TDC.)

ac9wzw00002235

9. Follow the “TIMING CHAIN REMOVAL/INSTALLATION” procedure and install the timing chain. (See TIMING CHAIN REMOVAL/INSTALLATION [MZI-3.7].)