SECOND-ROW CENTER SEAT BELT REMOVAL/INSTALLATION

id081100802400

  Caution
  • The ELR (emergency locking retractor) has a spring that will unwind if the retractor cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

1. Turn the ignition switch to the OFF position.

2. Disconnect the negative battery cable.

3. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (4) Front seat belt lower anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (5) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (6) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (7) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (8) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (9) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (10) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (11) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (12) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (13) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (14) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (15) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (16) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (17) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (18) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (19) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (20) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (21) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (22) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

4. Remove the bolt.

L.H.D.

ac9wzw00000951

R.H.D.

ac9wzw00000952

5. Remove the second-row center seat belt.

6. Install in the reverse order of removal.