FRONT BRAKE (DISC) REMOVAL/INSTALLATION

id041100800900

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, add brake fluid, bleed the air, and inspect for fluid leakage. (See AIR BLEEDING.)

4. After installation, depress the brake pedal a few times, rotate the wheel by hand, and verify that the brake does not drag.

ac9wzw00003017

1 | Brake hose
2 | Slide pin bolt
3 | Caliper (See Caliper Installation Note.)
4 | Disc pad
5 | Pad wear indicator
6 | Shim
7 | Guide plate
8 | Bolt
9 | Mounting support
10 | Dust boot
11 | Disc plate

Caliper Installation Note

1. Push the piston fully inward using the SST.

ac9wzw00000133

2. Install the caliper.