DTC B267B [POWER LIFTGATE (PLG) SYSTEM]

id0902e9381900

DTC B267B | Full latch switch circuit malfunction
--- | ---
DETECTION CONDITION | A short circuit to the ground system in the wiring harness between the liftgate latch and lock actuator and PLG control module.
POSSIBLE CAUSE | • Short to GND in wiring harness between PLG control module terminal 3G and liftgate latch and lock actuator terminal D • Full latch switch malfunction • PLG control module malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT WIRING HARNESS BETWEEN PLG CONTROL UNIT AND LIFTGATE LATCH AND LOCK ACTUATOR • Disconnect the PLG control module connector. • Disconnect the liftgate latch and lock actuator connector. • Inspect the wiring harness between PLG control module terminal 3G and liftgate latch and lock actuator terminal D for a short circuit to ground system. • Is the wiring harness normal? | Yes | Replace the liftgate latch and lock actuator. (See LIFTGATE LATCH AND LOCK ACTUATOR REMOVAL/INSTALLATION.) Go to the next step.
No | Repair or replace the wiring harness. Go to the next step.
2 | VERIFY CORRECTION COMPLETED • Reconnect the disconnected connector. • Clear the DTC. • Operate the PLG system. (Close operation) • Is DTC B267B stored? | Yes | Replace the PLG control module. (See POWER LIFTGATE (PLG) CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.