C-PILLAR TRIM REMOVAL/INSTALLATION

id091700802200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (6) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (7) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (8) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (9) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

3. Partially peel back the seaming welt.

4. Remove the cover in the direction of the arrow.

ac9uuw00000332

5. Remove the bolt.

ac9uuw00002129

6. Detach clip A and tab B, and pin C by pulling them in the direction of the arrow.

7. Remove the C-pillar trim.

8. Install in the reverse order of removal.