SIDE STEP MOLDING REMOVAL

id091600804400

1. Set the over fender out of the way. (See OVER FENDER REMOVAL/INSTALLATION.)

2. Remove the tow fasteners shown in the figure and set the front over fender out of the way.

ac9wzw00001426

3. Slide the side step molding in the direction of the arrow and detach clips A and B.

4. Remove the side step molding.

5. Remove clips A and B from the body, then install it to the side step molding.