SUPPLIER IDENTIFICATION PROCEDURE [AUDIO]

id0902f6803800

  Note
  • The unit supplier can vary. When asking the supplier (service center) for repair or replacement, identify the supplier and fill in the Audio Repair Order Form using the following procedures.

Verification procedure using label or inscribed lettering

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (2) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

3. Verify the supplier name by referring to the label attached to the unit.

ac5wzw00000726

1. Turn the ignition switch to the ACC or ON position.

2. Verify that the audio is turned on. If the audio is turned off, press the POWER/VOLUME button to turn it on.

3. Press the POWER/VOLUME button and SEEK button (up) simultaneously to launch the diagnostic assist function.

With RDS (radio data system)

ac9wzw00002927

Without RDS (radio data system)

ac9wzw00002999

4. Verify that the launched diagnostic assist function is displayed on the screen.

ac5jjw00001767

5. Input diagnostic assist code ”06”.

ac9wzw00002929

6. Select ”ENTER button”.

7. Identify the supplier code by referring to the display.

ac5jjw00001769

Supplier code | Supplier name
--- | ---
M-01 | SANYO Automedia
M-02 | Panasonic
M-03 | Clarion
M-04 | Pioneer
M-05 | VISTEON

8. Press the POWER/VOLUME button and return to the diagnostic assist screen.

ac5jjw00001767

9. Press the POWER/VOLUME button and end the diagnostic assist function.