DTC P065B:00 [MZI-3.7]

id0102d2315800

DTC P065B:00 | Generator control circuit range/performance
--- | ---
DETECTION CONDITION | • If the generator input frequency was continuously less than 80 Hz or more than 200 Hz the PCM will set this DTC.
POSSIBLE CAUSE | • Connector or terminal malfunction • Short to power supply between generator terminal LI and PCM terminal 1O • Short to ground between generator terminal LI and PCM terminal 1O • Open circuit between generator terminal LI and PCM terminal 1O • Generator malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT GENERATOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the generator connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Are there any malfunction? | Yes | Repair or replace suspected part, then go to Step 10.
No | Go to the next step.
4 | INSPECT GENERATOR CIRCUIT FOR SHORT TO POWER SUPPLY • Generator connector is disconnected. • Turn the ignition switch to the ON position (engine off). • Measure the voltage between generator terminal LI (wiring harness-side) and body ground. • Is the voltage B+? | Yes | Repair or replace suspected part, then go to Step 10.
No | Go to the next step.
5 | INSPECT GENERATOR CIRCUIT FOR SHORT TO GROUND • Generator connector is disconnected. • Inspect for continuity between generator terminal LI (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace suspected part, then go to the next step.
No | Go to the next step.
6 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Inspect for poor connection (such as damaged/pulled-out terminals, corrosion). • Are there any malfunction? | Yes | Repair or replace suspected part, then go to Step 10.
No | Go to the next step.
7 | INSPECT GENERATOR CIRCUIT FOR OPEN CIRCUIT • Generator and PCM connectors are disconnected. • Inspect for continuity between generator terminal LI (wiring harness-side) and PCM terminal 1O (wiring harness-side) • Is there continuity? | Yes | Go to the next step.
No | Repair or replace suspected part, then go to Step 10.
8 | INSPECT BATTERY POSITIVE TERMINAL FOR POOR INSTALLATION • Turn the ignition switch off. • Inspect the battery positive terminal for looseness. • Is there any malfunction? | Yes | Connect the battery positive terminal correctly, then go to Step 10.
No | Go to the next step.
9 | INSPECT GENERATOR • Inspect the generator. (See GENERATOR INSPECTION [MZI-3.7].) • Is there any malfunction? | Yes | Replace the generator, then go to the next step. (See GENERATOR REMOVAL/INSTALLATION [MZI-3.7].)
No | Go to the next step.
10 | VERIFY TROUBLESHOOTING OF DTC P065B:00 HAS BEEN COMPLETED • Verify that all disconnected connectors reconnected. • Clear the DTC from the PCM memory using the M-MDS. • Perform the KOEO or KOER self-test. (See KOEO/KOER SELF TEST [MZI-3.7].) • Is the PENDING CODE for this DTC present? | Yes | Repeat the inspection from Step 1. • If the malfunction recurs, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZI-3.7].) Go to the next step.
No | Go to the next step.
11 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [MZI-3.7].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZI-3.7].)
No | Troubleshooting completed.