GLOVE COMPARTMENT REMOVAL/INSTALLATION

id091700800700

  Caution
  • If the glove compartment is closed without being joined to the stay damper, the stay damper may be damaged. Verify that the stay damper is joined to the glove compartment before closing the glove compartment.

1. Remove the following parts:

  (1) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment service hole cover (See AIR FILTER REMOVAL/INSTALLATION.)

2. Pull the stay damper in the direction shown in the figure, and detach the connecting part between the glove compartment and the stay damper.

R.H.D.

ac9wzw00000210

L.H.D.

ac9uuw00002111

3. Insert fingers into the glove compartment service hole and detach the stoppers while holding the instrument panel.

R.H.D.

ac9wzw00000211

L.H.D.

ac9uuw00002112

4. Lower the glove compartment.

R.H.D.

ac9wzw00000212

L.H.D.

ac9uuw00002113

5. Detach the hook from the dashboard and remove the glove compartment.

6. Install in the reverse order of removal.