FRONT LOWER ARM REMOVAL/INSTALLATION

id021300800600

  Note
  • For this vehicle, a spacer is present/not present on the steering knuckle. After verifying whether the spacer is equipped or not, perform the removal/installation using the following procedure.
  • There is no problem with the left or right steering knuckle having either a spacer or no spacer.

1. When working on the left side of the vehicle, disconnect the front auto leveling sensor link lower side. (Vehicle with headlight auto leveling system) (See FRONT AUTO LEVELING SENSOR REMOVAL/INSTALLATION

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Inspect for front wheel alignment, and adjust it as necessary. (See FRONT WHEEL ALIGNMENT.)

ac9wzw00003275

1 | Stabilizer control link lower nut
2 | Front lower arm ball joint
3 | Front lower arm
4 | Spacer (With spacer)