POWER LIFTGATE (PLG) TOUCH SENSOR REMOVAL/INSTALLATION

id091100001100

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Liftgate upper trim (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION.)

  (2) PLG arm (See POWER LIFTGATE (PLG) DRIVE UNIT REMOVAL/INSTALLATION.)

  (3) Liftgate side trim (See LIFTGATE SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Liftgate lower trim (See LIFTGATE LOWER TRIM REMOVAL/INSTALLATION.)

3. Disconnect the PLG touch sensor connector.

ac9uuw00000896

4. Remove the screws.

5. Remove the PLG touch sensor.

6. Install in the reverse order of removal.