STARTER INSPECTION [MZI-3.7]

id0119c2800300

On-vehicle Inspection

1. Verify that the battery is fully charged.

2. The starter is normal if it rotates smoothly and without any noise when the engine is cranked.

  • If the starter does not operate, inspect the following:
    ― Remove the starter, and inspect the starter unit.
    ― Inspect the related wiring harnesses, the ignition switch, and the transaxle range switch.

No-load Test

1. Verify that the battery is fully charged.

2. Connect the starter, battery, and a tester as shown in the figure.

ac9wzw00002097

3. Operate the starter and verify that it rotates smoothly.

  • If the starter does not rotate smoothly, inspect the starter unit.

4. Measure the voltage and current while the starter is operating.

  • If not within the specification, replace the starter.

  Starter no-load test voltage

  11 V

  Starter no-load test current

  90 A or less

Magnetic Switch Operation Inspection

Pull-out test

  Note
  • Depending on the battery charge condition, the starter motor pinion may rotate while in an extended state. This is due to current flowing to the starter motor through the pull-in coil to turn the starter motor, and does not indicate an abnormality.

1. Verify that the starter motor pinion is extended while battery positive voltage is connected to terminal S and the starter body is grounded.

ac9wzw00002098

  • If the starter motor pinion is not extended, repair or replace the starter.

Return test

1. Disconnect the motor wire from terminal M.

2. Connect battery positive voltage to terminal M and ground the starter body.

ac9wzw00002099

3. Pull out the drive pinion with a screwdriver. Verify that it returns to its original position when released.

  • If it does not return, repair or replace the starter.

Pinion Gap Inspection

1. Pull out the drive pinion with the battery positive voltage connected to terminal S and the starter body grounded.

ac9wzw00002098

  Caution
  • Applying power for more than 10 s can damage the starter. Do not apply power for more than 10 s.

2. Measure the pinion gap while the drive pinion is extended.

ac9wzw00002100

  • If not as specified, adjust with an adjustment washer (between drive housing front cover and magnetic switch).

  Starter pinion gap

  0 mm {0 in}

Starter Inner Parts Inspection

Armature

1. Verify that there is no continuity between the commutator and the core at each segment using a tester.

ac9wzw00002101

  • If there is continuity, replace the armature.

2. Verify that there is no continuity between the commutator and the shaft using a tester.

ac9wzw00002102

  • If there is continuity, replace the armature.

3. Place the armature on V-blocks, and measure the runout using a dial indicator.

  • If it exceeds the maximum specification, replace the armature.

ac9wzw00002103

  Starter armature runout

  0.1 mm {0.004 in} max.

4. Measure the commutator diameter.

ac9wzw00002104

  • If not within the minimum specification, replace the armature.

  Starter commutator diameter

  Standard: 29.4 mm {1.16 in}
  Minimum: 28.8 mm {1.13 in}

5. Measure the segment groove depth of the commutator.

ac9wzw00002105

  • If not within the minimum specification, undercut the grooves to the standard depth.

  Segment groove depth of starter commutator

  Standard: 0.5 mm {0.02 in}
  Minimum: 0.2 mm {0.008 in}

Magnetic switch

1. Inspect for continuity between terminals S and M using a tester.

ac9wzw00002106

  • If there is no continuity, replace the magnetic switch.

2. Inspect for continuity between terminal S and the body using a tester.

ac9wzw00002107

  • If there is no continuity, replace the magnetic switch.

3. Verify that there is no continuity between terminals M and B using a tester.

ac9wzw00002108

  • If there is continuity, replace the magnetic switch.

Brush and brush holder

1. Verify that there is no continuity between each insulated brush and plate using a tester.

ac9wzw00002109

  • If there is continuity, replace the brush holder.

2. Measure the brush length.

ac9wzw00002110

  • If any brush is worn almost to or beyond the minimum specification, replace all of the brushes.

  Starter brush length

  Standard: 12.3 mm {0.48 in}
  Minimum: 5.5 mm {0.22 in}

3. Measure the brush spring force using a spring balance.

ac9wzw00002111

  • If not within the minimum specification, replace the brush and brush holder component.

  Starter brush spring force

  Standard: 15.0—20.4 N {1.53—2.08 kgf, 3.38—4.58 lbf}
  Minimum: 2.75 N {0.28 kgf, 0.62 lbf}