DSC INDICATOR LIGHT OPERATION

id041800820200

• When the dynamic stability control (DSC)/roll stability control (RSC) and controller area network (CAN) lines are normal, the DSC indicator light illuminates for approx. 3 s when the ignition switch is turned to the ON position to check the light function. When the system is malfunctioning, the DSC indicator light remains illuminated.
• When the RSC or DSC or traction control system (TCS) is operating (RSC/DSC/TCS has not been disabled by pressing the TCS OFF switch), the DSC indicator light operates as follows:

DSC Indicator Light Operation

Item | DSC indicator light condition
TCS, DSC, RSC not operating | Not illuminated
TCS operating | Flashes (0.5 s intervals)
DSC operating
RSC operating

ac9wzn00000284