MIRROR BASE REMOVAL

id091200005300

1. Remove the rearview mirror. (See REARVIEW MIRROR REMOVAL.)

2. Wind each end of a wire around a bar.

ac9wzw00001691

  Warning
  • Using the piano wire with bare hands can cause injury. Always wear gloves when using the piano wire.

  Note
  • Use a long sawing action to spread the work over the whole length of the piano wire to prevent it from breaking.

3. Fix one end of the piano wire, and while pulling the other end, cut the sealant to remove the base.