REAR OUTER HANDLE REMOVAL/INSTALLATION

id091400803200

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Inner sail garnish (See INNER SAIL GARNISH REMOVAL/INSTALLATION.)

  (2) Rear door trim (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

  (3) Rear door speaker (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

  (4) Rear door glass (See REAR DOOR GLASS REMOVAL/INSTALLATION.)

  (5) Rear door module (See REAR DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove the service hole cover.

4. Remove the fastener.

ac9uuw00001290

5. Remove the shock-absorbing pad.

6. Disconnect the rod.

7. Remove the nuts.

8. Remove the handle base.

9. Remove the bolts.

10. Secure the rear part of the rear outer handle and, with the rear outer handle lever pulled outward (1), remove the rear part of the rear outer handle from the rear door.

acxuuw00002480

11. Install in the reverse order of removal.